<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<text>Red</text>
<text>Green</text>
<text>Blue</text>
<text>Hue</text>
<text>Saturation</text>
<text>Value</text>
<text>RGB</text>
<text>HSV</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>D9</text>
<text>Evil Genius Labs</text>
<text>FastLED RGB &amp; HSV</text>
<text>evilgeniuslabs.org</text>
<text>Teensy LC</text>
<text>Red/Hue Pot</text>
<text>Green/Sat Pot</text>
<text>Blue/Val Pot</text>
<text>Button</text>
<text>Switch</text>
<text>LED0</text>
<text>USB</text>
<text>USB</text>
<text>Rainbows!</text>
<text>GND</text>
<text>5V</text>
<text>D17</text>
<text>GND</text>
<wire x1="36.195" y1="47.14875" x2="1.5875" y2="47.14875" width="0" layer="20"/>
<wire x1="1.5875" y1="47.14875" x2="0.3175" y2="45.87875" width="0" layer="20" curve="90"/>
<wire x1="0.3175" y1="45.87875" x2="0.3175" y2="1.27" width="0" layer="20"/>
<wire x1="0.3175" y1="1.27" x2="1.5875" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.5875" y1="0" x2="36.195" y2="0" width="0" layer="20"/>
<wire x1="36.195" y1="0" x2="37.465" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="37.465" y1="45.87875" x2="36.195" y2="47.14875" width="0" layer="20" curve="90"/>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>D2</text>
<text>D9</text>
<text>D17</text>
<text>v0.1 2017</text>
<wire x1="37.465" y1="45.87875" x2="37.465" y2="1.27" width="0" layer="20"/>
</plain>
<libraries>
<library name="Bourns">
<packages>
<package name="PTV09A-4">
<description>PTV09 Series -9mm Potentiometer Vertical</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X05">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.1EZ">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="EG1218">
</package>
</packages>
</library>
<library name="switch-omron">
<description>&lt;b&gt;Omron Switches&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B3F-10XX">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Teensy_3_and_LC_Series_Boards_v1.1">
<packages>
<package name="TEENSY3-DIL">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V-KIT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="B-S-POT" library="Bourns" package="PTV09A-4" value="B-S-POT"/>
<element name="G-S-POT" library="Bourns" package="PTV09A-4" value="G-S-POT"/>
<element name="R-H-POT" library="Bourns" package="PTV09A-4" value="R-H-POT"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.1EZ" value="300-500Ω">
<attribute name="VALUE"/>
</element>
<element name="SPDT" library="adafruit" package="EG1218" value="SPDT">
<attribute name="NAME"/>
</element>
<element name="D2" library="switch-omron" package="B3F-10XX" value="D2">
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="176432"/>
<attribute name="OC_NEWARK" value="36M3542"/>
<attribute name="MPN" value="B3F-1000"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.1EZ" value="10KΩ">
<attribute name="VALUE"/>
</element>
<element name="TEENSYLC" library="Teensy_3_and_LC_Series_Boards_v1.1" package="TEENSY3-DIL" value="TEENSY_LC_DIL"/>
<element name="U$3" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="LED" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Electromechanical" package="STAND-OFF" value=""/>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-10UF-25V-KIT" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R-H-POT" pad="1"/>
<contactref element="G-S-POT" pad="1"/>
<contactref element="B-S-POT" pad="1"/>
<contactref element="SPDT" pad="O"/>
<contactref element="R2" pad="P$1"/>
<contactref element="TEENSYLC" pad="GND"/>
<contactref element="TEENSYLC" pad="AGND"/>
<contactref element="LED" pad="1"/>
<contactref element="LED" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="P0">
<contactref element="R-H-POT" pad="2"/>
<contactref element="TEENSYLC" pad="14/A0"/>
</signal>
<signal name="P1">
<contactref element="G-S-POT" pad="2"/>
<contactref element="TEENSYLC" pad="15/A1"/>
</signal>
<signal name="P2">
<contactref element="B-S-POT" pad="2"/>
<contactref element="TEENSYLC" pad="16/A2"/>
</signal>
<signal name="LED0">
<contactref element="R1" pad="P$2"/>
<contactref element="LED" pad="2"/>
</signal>
<signal name="R1">
<contactref element="R1" pad="P$1"/>
<contactref element="TEENSYLC" pad="17/A3"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="B1">
<contactref element="SPDT" pad="P"/>
<contactref element="TEENSYLC" pad="9"/>
</signal>
<signal name="N$1">
<contactref element="D2" pad="1"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="S1">
<contactref element="D2" pad="2"/>
<contactref element="TEENSYLC" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="TEENSYLC" pad="VIN"/>
<contactref element="LED" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="TEENSYLC" pad="3.3V"/>
<contactref element="D2" pad="3"/>
<contactref element="SPDT" pad="S"/>
<contactref element="B-S-POT" pad="3"/>
<contactref element="G-S-POT" pad="3"/>
<contactref element="R-H-POT" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
